
    =========================== USB Port2 ===========================

Connection Status        : 0x01 (Device is connected)
Port Chain               : 1-2
Properties               : 0x01
 IsUserConnectable       : yes
 PortIsDebugCapable      : no
 PortHasMultiCompanions  : no
 PortConnectorIsTypeC    : no
ConnectionIndex          : 2
CompanionIndex           : 0
 CompanionHubSymLnk      : U
 CompanionPortNumber     : 14

      ======================== USB Device ========================

        +++++++++++++++++ Device Information ++++++++++++++++++
Device Description       : USB-Eingabegerät
Device Path              : \\?\usb#vid_16d0&pid_0830#1000000000000001#{a5dcbf10-6530-11d2-901f-00c04fb951ed}
Device ID                : USB\VID_16D0&PID_0830\1000000000000001
Hardware IDs             : USB\VID_16D0&PID_0830&REV_0103 USB\VID_16D0&PID_0830
Driver KeyName           : {745a17a0-74d3-11d0-b6fe-00a0c90f57da}\0018 (GUID_DEVCLASS_HIDCLASS)
Driver                   : \SystemRoot\System32\drivers\hidusb.sys (Version: 10.0.17134.1  Date: 2018-04-12)
Driver Inf               : C:\WINDOWS\inf\input.inf
Legacy BusType           : PNPBus
Class                    : HIDClass
Class GUID               : {745a17a0-74d3-11d0-b6fe-00a0c90f57da} (GUID_DEVCLASS_HIDCLASS)
Interface GUID           : {a5dcbf10-6530-11d2-901f-00c04fb951ed} (GUID_DEVINTERFACE_USB_DEVICE)
Service                  : HidUsb
Enumerator               : USB
Location Info            : Port_#0002.Hub_#0001
Location IDs             : PCIROOT(0)#PCI(1400)#USBROOT(0)#USB(2), ACPI(_SB_)#ACPI(PCI0)#ACPI(XHC_)#ACPI(RHUB)#ACPI(HS02)
Container ID             : {7e7c5f09-0365-5278-ba33-1a9e097cd624}
Manufacturer Info        : (Standardsystemgeräte)
Capabilities             : 0x94 (Removable, UniqueID, SurpriseRemovalOK)
Status                   : 0x0180600A (DN_DRIVER_LOADED, DN_STARTED, DN_DISABLEABLE, DN_REMOVABLE, DN_NT_ENUMERATOR, DN_NT_DRIVER)
Problem Code             : 0
Power State              : D0 (supported: D0, D3, wake from D0)
 Child Device 1          : HID-konformes, vom Hersteller definiertes Gerät
  DevicePath             : \\?\hid#vid_16d0&pid_0830#6&f1ea06f&1&0000#{4d1e55b2-f16f-11cf-88cb-001111000030}
  KernelName             : \Device\000002d9
  Device ID              : HID\VID_16D0&PID_0830\6&F1EA06F&1&0000
  Class                  : HIDClass

        ---------------- Connection Information ---------------
Connection Index         : 0x02 (2)
Connection Status        : 0x01 (DeviceConnected)
Current Config Value     : 0x01
Device Address           : 0x12 (18)
Is Hub                   : 0x00 (no)
Number Of Open Pipes     : 0x02 (2)
Device Bus Speed         : 0x01 (Full-Speed)
Pipe0ScheduleOffset      : 0x00 (0)
Pipe1ScheduleOffset      : 0x00 (0)
Data (HexDump)           : 02 00 00 00 12 01 10 01 00 00 00 08 D0 16 30 08   ..............0.
                           03 01 01 02 03 01 01 01 00 12 00 02 00 00 00 01   ................
                           00 00 00 07 05 81 03 21 00 01 00 00 00 00 07 05   .......!........
                           02 03 21 00 01 00 00 00 00                        ..!......

        --------------- Connection Information V2 -------------
Connection Index         : 0x02 (2)
Length                   : 0x10 (16 bytes)
SupportedUsbProtocols    : 0x03
 Usb110                  : 1 (yes)
 Usb200                  : 1 (yes)
 Usb300                  : 0 (no)
 ReservedMBZ             : 0x00
Flags                    : 0x00
 DevIsOpAtSsOrHigher     : 0 (Is not operating at SuperSpeed or higher)
 DevIsSsCapOrHigher      : 0 (Is not SuperSpeed capable or higher)
 DevIsOpAtSsPlusOrHigher : 0 (Is not operating at SuperSpeedPlus or higher)
 DevIsSsPlusCapOrHigher  : 0 (Is not SuperSpeedPlus capable or higher)
 ReservedMBZ             : 0x00
Data (HexDump)           : 02 00 00 00 10 00 00 00 03 00 00 00 00 00 00 00   ................

    ---------------------- Device Descriptor ----------------------
bLength                  : 0x12 (18 bytes)
bDescriptorType          : 0x01 (Device Descriptor)
bcdUSB                   : 0x110 (USB Version 1.10)
bDeviceClass             : 0x00 (defined by the interface descriptors)
bDeviceSubClass          : 0x00
bDeviceProtocol          : 0x00
bMaxPacketSize0          : 0x08 (8 bytes)
idVendor                 : 0x16D0
idProduct                : 0x0830
bcdDevice                : 0x0103
iManufacturer            : 0x01 (String Descriptor 1)
 Language 0x0409         : "DMXControl Projects e.V."
iProduct                 : 0x02 (String Descriptor 2)
 Language 0x0409         : "Nodle U1"
iSerialNumber            : 0x03 (String Descriptor 3)
 Language 0x0409         : "1000000000000001"
bNumConfigurations       : 0x01 (1 Configuration)
Data (HexDump)           : 12 01 10 01 00 00 00 08 D0 16 30 08 03 01 01 02   ..........0.....
                           03 01                                             ..

    ------------------ Configuration Descriptor -------------------
bLength                  : 0x09 (9 bytes)
bDescriptorType          : 0x02 (Configuration Descriptor)
wTotalLength             : 0x0029 (41 bytes)
bNumInterfaces           : 0x01 (1 Interface)
bConfigurationValue      : 0x01 (Configuration 1)
iConfiguration           : 0x00 (No String Descriptor)
bmAttributes             : 0x80
 D7: Reserved, set 1     : 0x01
 D6: Self Powered        : 0x00 (no)
 D5: Remote Wakeup       : 0x00 (no)
 D4..0: Reserved, set 0  : 0x00
MaxPower                 : 0x64 (200 mA)
Data (HexDump)           : 09 02 29 00 01 01 00 80 64 09 04 00 00 02 03 00   ..).....d.......
                           00 00 09 21 10 01 00 01 22 24 00 07 05 81 03 21   ...!...."$.....!
                           00 01 07 05 02 03 21 00 01                        ......!..

        ---------------- Interface Descriptor -----------------
bLength                  : 0x09 (9 bytes)
bDescriptorType          : 0x04 (Interface Descriptor)
bInterfaceNumber         : 0x00
bAlternateSetting        : 0x00
bNumEndpoints            : 0x02 (2 Endpoints)
bInterfaceClass          : 0x03 (HID - Human Interface Device)
bInterfaceSubClass       : 0x00 (None)
bInterfaceProtocol       : 0x00 (None)
iInterface               : 0x00 (No String Descriptor)
Data (HexDump)           : 09 04 00 00 02 03 00 00 00                        .........

        ------------------- HID Descriptor --------------------
bLength                  : 0x09 (9 bytes)
bDescriptorType          : 0x21 (HID Descriptor)
bcdHID                   : 0x0110 (HID Version 1.10)
bCountryCode             : 0x00 (00 = not localized)
bNumDescriptors          : 0x01
Data (HexDump)           : 09 21 10 01 00 01 22 24 00                        .!...."$.
Descriptor 1:
bDescriptorType          : 0x22 (Class=Report)
wDescriptorLength        : 0x0024 (36 bytes)
Error reading descriptor : ERROR_INVALID_PARAMETER

        ----------------- Endpoint Descriptor -----------------
bLength                  : 0x07 (7 bytes)
bDescriptorType          : 0x05 (Endpoint Descriptor)
bEndpointAddress         : 0x81 (Direction=IN EndpointID=1)
bmAttributes             : 0x03 (TransferType=Interrupt)
wMaxPacketSize           : 0x0021 (33 bytes)
bInterval                : 0x01 (1 ms)
Data (HexDump)           : 07 05 81 03 21 00 01                              ....!..

        ----------------- Endpoint Descriptor -----------------
bLength                  : 0x07 (7 bytes)
bDescriptorType          : 0x05 (Endpoint Descriptor)
bEndpointAddress         : 0x02 (Direction=OUT EndpointID=2)
bmAttributes             : 0x03 (TransferType=Interrupt)
wMaxPacketSize           : 0x0021 (33 bytes)
bInterval                : 0x01 (1 ms)
Data (HexDump)           : 07 05 02 03 21 00 01                              ....!..

      -------------------- String Descriptors -------------------
             ------ String Descriptor 0 ------
bLength                  : 0x04 (4 bytes)
bDescriptorType          : 0x03 (String Descriptor)
Language ID[0]           : 0x0409 (English - United States)
Data (HexDump)           : 04 03 09 04                                       ....
             ------ String Descriptor 1 ------
bLength                  : 0x32 (50 bytes)
bDescriptorType          : 0x03 (String Descriptor)
Language 0x0409          : "DMXControl Projects e.V."
Data (HexDump)           : 32 03 44 00 4D 00 58 00 43 00 6F 00 6E 00 74 00   2.D.M.X.C.o.n.t.
                           72 00 6F 00 6C 00 20 00 50 00 72 00 6F 00 6A 00   r.o.l. .P.r.o.j.
                           65 00 63 00 74 00 73 00 20 00 65 00 2E 00 56 00   e.c.t.s. .e...V.
                           2E 00                                             ..
             ------ String Descriptor 2 ------
bLength                  : 0x12 (18 bytes)
bDescriptorType          : 0x03 (String Descriptor)
Language 0x0409          : "Nodle U1"
Data (HexDump)           : 12 03 4E 00 6F 00 64 00 6C 00 65 00 20 00 55 00   ..N.o.d.l.e. .U.
                           31 00                                             1.
             ------ String Descriptor 3 ------
bLength                  : 0x22 (34 bytes)
bDescriptorType          : 0x03 (String Descriptor)
Language 0x0409          : "1000000000000001"
Data (HexDump)           : 22 03 31 00 30 00 30 00 30 00 30 00 30 00 30 00   ".1.0.0.0.0.0.0.
                           30 00 30 00 30 00 30 00 30 00 30 00 30 00 30 00   0.0.0.0.0.0.0.0.
                           31 00                                             1.
